# Quang Nguyen – Hw # 3

2/11/2016

The maximum frequency that I was able to use and still meet the design requirement is , which give me a worst negative slack of 3.559 ns.